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	Paper-feeding part is operated by a single board and regulated quickly and simply. Distances between papers are adjusted by the imported segmentless adjustor and vibrant engine is set to make the sending part more stable. In ready -folding part, the first fold and the third fold can be exchanged by 180 degree or 90 degree. The second fold and the fourth fold can be molded in 180 degree, which is easy for the automatic packing production lines to mold the pack boxes. In additional, we can increase the ready-folding of 180 degree -135 degree.
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